**EXPERIMENT 2**

Using your choice for IDE, get the servo to move 45, 90, 120 degrees.

*Description*: The pulse length, defined as a uint16\_t data type (16 bit unsigned integer) defines the angle position of the servo. After a few tests on possible values, the ones for 45, 90, and 120 is defined as shown in the code.

