**EXPERIMENT 1**

Use an assortment of bitmaps to get four LEDs connected to PORTB to continuously come on and off in ascending order.

*Description*: Bit twiddling is used to set bits on pins that corresponds to the LED that is desired to light up. Those pins sends voltage to the LEDs to light them up.

